ABC/HR Version 1.1 beta 2, 18 June 2004
Testname: 

1L = D:\lame test\ff123 suite\096 kbps\bonus\dogies [3.90.3 - ABR - 096].wav
2L = D:\lame test\ff123 suite\096 kbps\bonus\dogies [3.97a5 - VBR - V8].wav
3L = D:\lame test\ff123 suite\096 kbps\bonus\dogies [3.96.1 - ABR - 096].wav
4L = D:\lame test\ff123 suite\096 kbps\bonus\dogies [3.97a5 - ABR - 096 - XX10].wav
5L = D:\lame test\ff123 suite\096 kbps\bonus\dogies [3.97a5 - VBR - V7].wav

---------------------------------------
General Comments:

---------------------------------------
1L File: D:\lame test\ff123 suite\096 kbps\bonus\dogies [3.90.3 - ABR - 096].wav
1L Rating: 2.5
1L Comment: 
---------------------------------------
2L File: D:\lame test\ff123 suite\096 kbps\bonus\dogies [3.97a5 - VBR - V8].wav
2L Rating: 1.2
2L Comment: 
---------------------------------------
3L File: D:\lame test\ff123 suite\096 kbps\bonus\dogies [3.96.1 - ABR - 096].wav
3L Rating: 1.4
3L Comment: very similar if not the same as 2L... up to 00:04.500. Then, brass is severly distorted (boiling oil sound).
---------------------------------------
4L File: D:\lame test\ff123 suite\096 kbps\bonus\dogies [3.97a5 - ABR - 096 - XX10].wav
4L Rating: 2.5
4L Comment: 
---------------------------------------
5L File: D:\lame test\ff123 suite\096 kbps\bonus\dogies [3.97a5 - VBR - V7].wav
5L Rating: 2.0
5L Comment: 
---------------------------------------
ABX Results:
D:\lame test\ff123 suite\096 kbps\bonus\dogies [3.90.3 - ABR - 096].wav vs D:\lame test\ff123 suite\096 kbps\bonus\dogies [3.97a5 - ABR - 096 - XX10].wav
    2 out of 8, pval = 0.965
