ABC/HR for Java, Version 0.5a, 17 août 2005
Testname: 

Tester: guruboolez

1R = E:\SUMMER TESTS 2005\HQ180\09_Orion II [AAC faac].wav
2L = E:\SUMMER TESTS 2005\HQ180\09_Orion II [MPC 1.15v].wav
3L = E:\SUMMER TESTS 2005\HQ180\09_Orion II [MP3 LAME].wav
4L = E:\SUMMER TESTS 2005\HQ180\09_Orion II [vorbis aoTuV].wav
5L = E:\SUMMER TESTS 2005\HQ180\09_Orion II [AAC Nero Digital].wav

---------------------------------------
General Comments: 
---------------------------------------
1R File: E:\SUMMER TESTS 2005\HQ180\09_Orion II [AAC faac].wav
1R Rating: 3.3
1R Comment: There's noise covering the microattacks which are slightly blurred.
---------------------------------------
2L File: E:\SUMMER TESTS 2005\HQ180\09_Orion II [MPC 1.15v].wav
2L Rating: 3.8
2L Comment: Noise between micro-attacks. Not really annoying, but clearly perceptible.
AFTER ABX: there's a clear 'pshhhhh-artefact' that identifies this encoding when compared directly to 4L.
---------------------------------------
3L File: E:\SUMMER TESTS 2005\HQ180\09_Orion II [MP3 LAME].wav
3L Rating: 3.0
3L Comment: Noise is higher than 1R. Noise reachs a peak somewhere between 3.90 - 6.67.
---------------------------------------
4L File: E:\SUMMER TESTS 2005\HQ180\09_Orion II [vorbis aoTuV].wav
4L Rating: 4.0
4L Comment: Blurring and noise; better than 1R & 3R, very similar to 2L.
AFTER ABX: this one is cleaner compared to 2L. No artefact here, just a slight constant noise.
---------------------------------------
5L File: E:\SUMMER TESTS 2005\HQ180\09_Orion II [AAC Nero Digital].wav
5L Rating: 1.0
5L Comment: Very ugly distortion. Micro-attacks are slaughtered. It's very annoying, and 1.0 isn't severe at all.
---------------------------------------

ABX Results:
E:\SUMMER TESTS 2005\HQ180\09_Orion II [MPC 1.15v].wav vs E:\SUMMER TESTS 2005\HQ180\09_Orion II [vorbis aoTuV].wav
    12 out of 12, pval < 0.001
Original vs E:\SUMMER TESTS 2005\HQ180\09_Orion II [MPC 1.15v].wav
    14 out of 16, pval = 0.0020
Original vs E:\SUMMER TESTS 2005\HQ180\09_Orion II [vorbis aoTuV].wav
    13 out of 16, pval = 0.01


---- Detailed ABX results ----
E:\SUMMER TESTS 2005\HQ180\09_Orion II [MPC 1.15v].wav vs E:\SUMMER TESTS 2005\HQ180\09_Orion II [vorbis aoTuV].wav
Playback Range: 03.875 to 05.639
    11:31:21 PM p 1/1 pval = 0.5
    11:31:29 PM p 2/2 pval = 0.25
    11:31:32 PM p 3/3 pval = 0.125
    11:31:35 PM p 4/4 pval = 0.062
    11:31:38 PM p 5/5 pval = 0.031
    11:31:41 PM p 6/6 pval = 0.015
    11:31:43 PM p 7/7 pval = 0.0070
    11:31:46 PM p 8/8 pval = 0.0030
    11:31:49 PM p 9/9 pval = 0.0010
    11:31:52 PM p 10/10 pval < 0.001
    11:31:55 PM p 11/11 pval < 0.001
    11:31:58 PM p 12/12 pval < 0.001

Original vs E:\SUMMER TESTS 2005\HQ180\09_Orion II [MPC 1.15v].wav
Playback Range: 03.904 to 06.150
    11:26:14 PM p 1/1 pval = 0.5
    11:26:18 PM f 1/2 pval = 0.75
    11:26:22 PM p 2/3 pval = 0.5
    11:26:25 PM p 3/4 pval = 0.312
    11:26:28 PM p 4/5 pval = 0.187
    11:26:30 PM p 5/6 pval = 0.109
    11:26:34 PM p 6/7 pval = 0.062
    11:26:38 PM p 7/8 pval = 0.035
    11:26:42 PM p 8/9 pval = 0.019
    11:26:45 PM p 9/10 pval = 0.01
    11:26:49 PM p 10/11 pval = 0.0050
    11:26:53 PM p 11/12 pval = 0.0030
    11:26:58 PM p 12/13 pval = 0.0010
    11:27:02 PM f 12/14 pval = 0.0060
    11:27:06 PM p 13/15 pval = 0.0030
    11:27:10 PM p 14/16 pval = 0.0020

Original vs E:\SUMMER TESTS 2005\HQ180\09_Orion II [vorbis aoTuV].wav
Playback Range: 03.904 to 06.150
    11:28:21 PM p 1/1 pval = 0.5
    11:28:24 PM p 2/2 pval = 0.25
    11:28:27 PM f 2/3 pval = 0.5
    11:28:30 PM p 3/4 pval = 0.312
    11:28:33 PM p 4/5 pval = 0.187
    11:28:39 PM p 5/6 pval = 0.109
    11:28:42 PM p 6/7 pval = 0.062
    11:28:49 PM p 7/8 pval = 0.035
    11:28:51 PM f 7/9 pval = 0.089
    11:29:15 PM p 8/10 pval = 0.054
    11:29:21 PM p 9/11 pval = 0.032
    11:29:27 PM p 10/12 pval = 0.019
    11:29:31 PM p 11/13 pval = 0.011
    11:29:34 PM p 12/14 pval = 0.0060
    11:29:40 PM p 13/15 pval = 0.0030
    11:29:44 PM f 13/16 pval = 0.01

